***************************************************************************
Release notes for Vigor3300V

	Firmware Version 	: 2.6.3.0 (Release)
	Released Date		: 24th August 2010
	Build Date		: 18th August 2010
	Applicable Models	: Vigor3300V
	Locale			: UK Only

***************************************************************************

Important Notes
-----------------------

- Upgrade firmware should be carried out by suitably informed/experienced persons. 
- Backup your router configuration BEFORE upgrading firmware
- Upgrading Vigor3300V firmware using the .all file will retain your existing router settings.  
- If in doubt, consult your dealer firstly.


[New Features]
1. Support for AES192 and AES256 on IPSec phase I.
2. Added "Comment" field to IP Filter rules.
3. GlobalView WCF license can now be activated from the WAN side.

[Improvement]
1. Fixed: NAT session numbers are different between Data Flow monitor and NAT Session table.
2. Fixed: Ringing timer error when FXS module is 1005~1008.
3. Fixed: Could not change password from the router's web interface. The previous workaround was to set via telnet
4. Fixed: Resolved an issue with the router using the primary DNS IP to resolve Domain for HTTP Request Detection only.
5. Fixed: Possible connection problem when connecting a PC to a LAN port.
6. Improved: Added "Port Number" to the user access syslog output.
7. Improved: Added an option to enable or disable SNMP.
8. Improved: The TCP and UDP session timeouts can now be adjusted.


***************************************************************************
Release notes for Vigor3300V

	Firmware Version 	: 2.6.2.0 (Release)
	Released Date		: 15th June 2010
	Build Date		: 9th June 2010
	Applicable Models	: Vigor3300V
	Locale			: UK Only

***************************************************************************

New Features
1. Added “always on” feature for PPPoE WAN connections.
2. Added MAC address information to user access syslog output.
3. Added new telnet command, "ip bindmac show".
4. Support for Strato DDNS provider.
5. Support for GlobalView
6. Support for mOTP authentication for VPN users.

[Improvement]
1. Improved: IP verification mechanism in the WEB IP field.
2. Fixed: DHCP Over IPSec issue.
3. Fixed: Hotline did not work correctly in some circumstances.
4. Fixed: WAN Status display error.
5. Fixed: FXO packet detection problem


***************************************************************************
Release notes for Vigor3300V

	Firmware Version 	: 2.6.1.0 (Release)
	Released Date		: 24th November 2009
	Build Date		: 1st June 2009
	Applicable Models	: Vigor3300V
	Locale			: UK Only

***************************************************************************

[New Features]
Note: The reporting of the following logs can be enabled / disabled via Syslog:
Firewall, VPN, User Access, Call, WAN

[Improvement]
1. Support 100 nodes for Smart Monitor
2. Support NetBIOS over IPSec.
3. Add 90 ms and 120 ms code rate on VoIP Codec.
4. Add default WAN-IP address in address mapping.
5. Synchronize the configuration on HA.
6. Fix NAT loop backup problem when using 802.1q on LAN.
7. Improve VoIP Performance. VoIP won't be affected by network traffic.
8. Reduce CPU loading when 8 VoIP ports work at the same time.

[Known Issue]
1. FXO hotline feature is not working correctly. Will be fixed next version.
2. For VPN clients, DHCP over IPSec not working. VPN clients can still use traditional IPSec instead. Will be fixed next version.


***************************************************************************
Release notes for Vigor3300V

	Firmware Version 	: 2.6.0.0
	Released Date		: 24th November 2009
	Build Date		: 1st June 2009
	Applicable Models	: Vigor3300V
	Locale			: UK Only

***************************************************************************

[New Features]

1. Support aggressive mode for IPSEC VPN
2. Play congestion tone while receiving MWI message
3. Add intercall PIN code function
4. Add VigorDDNS
5. Append WAN default IP to address mapping option
6. Append an option for user to create IPSEC route 

[Improvements]

1. Enable/Disable packet forwarding between VLANs
2. Remove surfcontrol logo for all of the webpages
3. Corrected: tone web problem, and restart VoIP after configuring tone setting
4. Corrected: PIN code on-net causes system crash if wrong PIN code is typed
5. Corrected: hotline not working while PIN code enabled

***************************************************************************

Product Model      : Vigor3300V
Locale                 : UK Only
Firmware Version :  2.5.9.0
Release Type       : Formal Release
Released             :24th February 2009

***************************************************************************

Improvements in this firmware:

[New Features]
1. Support gratiutous ARP packet
2. Support 802.1Q VLAN on WAN interface
3. Support DDNS service "huagai.net"
4. Support adjustable MTU value for IPSEC
5. Support IP unnumbered function for IP routing
6. Support MS-CHAP, MS-CHAPv2 and MPPE for PPPoE/PPTP dial out
7. User access log added to syslog reporting
8. Support strict bind interface mechanism in load balance policy
9. Added enable / disable toggle for the data flow monitor
10. Support "nas-ip-address" and "nas-identifier" fields in RADIUS authentication packets
11. Added high availability function for 802.1Q VLAN on LAN interface
12. Added VoIP pin code for
13. Added watchdog function for IPSEC VPN
14. RIP protocol supported on WAN interface
15. Add 4 IVR tone files in flash (for pin code authentication) and verify them during system initial


[Fixed Issues]
1. Display Multi-LAN status on Webpage
2. Display correct ARP list in bind IP to MAC page
3. Display limit Session amount when using session limitation
4. Reduce the memory utilization
5. Increase the number of exceptions in contact filter (32 entries)
6. Create VPN route rule after IPSec tunnel connected
7. Automatically change the IP range of DHCP when LAN IP has been modified

[Modifications]
1. Modified flash partition and created a space to store tone files
2. Modified time unit of "FXO disconnect if no packet"
3. Modified input format for detination IP/mask in load balance policy
4. Modified input format for subnet mask for static route menu
5. Modified Remote Subnet IP to display correctly in IPSec VPN Status
6. Modified CPA surf control function to pass URL request when CPA server can not connect
7. Remove activate trial and purchase licence hyperlink in Web Content Filter
8. Renamed fields in data flow monitor 
9. Fixed DDNS status error when WAN port disconnects

Product Model      : Vigor3300V
Locale                 : UK Only
Firmware Version :  2.5.8
Release Type       : Formal Release
Released             : 10th April 2008

Improvements in this firmware:

[New features]
1.VPN Load-balance and backup.
2.Data Monitoring for LAN. 
3.Add hidden CLI command "wan_count" to change total wan count to 3 WAN or 4 WAN.
4.Add mtu setup option for static WAN for Vigor3300 series.
5.Add DNS option in VPN-> pptp general setup page for vigor3300/V.
6.Play dial tone only when port registered (selectable)
7.Add call waiting option function.

[Fixed issues]
1.Modify flash driver for ST, upgarde old firmware not support ST flash on device 
  with ST flash will be rejected.
2."Port Scan detection" causes host-to-lan ipsec unstable.
3.Address IPSEC DPD issue between multi sa.
4.Write log file prior to record SIP syslog. 
7.Fixed call hold failure issue. 
8.fix User can not use VoIP calling while IP only is bound with LAN issue.
9. Allow static dhcp setting more than 67.
10.Move Static DHCP function to Bind IP to MAC.
11.IPSec DPD can't drop a dead connection.
12.Fix dhcp server assign ip issue when enable strict bind in bind ip to mac.
13.Add index to diagnostic tool both in web and CLI.
14.Display NAT total sessions correctly in web.



Product Model      : Vigor3300V
Locale                 : UK Only
Firmware Version :  2.5.7.5
Release Type       : Formal Release
Released             : 3rd December 2007


Improvements in this firmware:

[Fixed issues]
1. Fix an issue for WUI in other languages
2.Fix IPSEC failure when PPPoE goes down/up momentarily
3.Fix DHCP server assigning duplicate IP to host. 
4.Prevent router reboot when enable CPA for the first time


Product Model    : Vigor3300V
Locale           : UK Only
Firmware Version :  2.5.7.4
Release Type     : Formal Release
Released         : 13th August 2007

Changes Since Firmware 2.5.7.1
---------------------------------

[New features]
1. Add Bypass(Normal Mode) FAX mode.  The original "Bypass fax mode" change to Bypass Proprietary FAX mode.    This mode only for 2 Vigor3300V proprietary using.
2. Add user can change User-Agent Name Function.   This function can let user change User-Agent Name at V3300V,   default value is "Draytek V3300V-1.0.0".
3. Add Call without Registration Function.   It will not sent REGISTER request while "Call without Registration" is set in per port setting.
4. Modify response for SIP NOTIFY.   Modify response with 200 OK when receive SIP NOTIFY.
5. Modify Porland CallerID.   Modify Porland CallerID Type DTMF to ETSI.
6. Add line reversal on both mode.   It can do Line Reversal both callee on hook and callee answer mode.
7. Add Call Waiting feature.

[Fixed issues]
1.Vigor 3300V NAT address mapping bug for PPPoE mode.
2.Fix SIP use intercall while Network failed issue.   Fix SIP can not use intercall while SIP using outbound proxy to make call.
3.Fix ddos issue, router have low throughput when attacked by flooding,    even enable ddos syn flood.
4.Enable multiple WAN and 802.1q VLAN, router cannot reset by web page.
5.Fix WAN DHCP issue, fail to get ip from Netgear WGR614v5 Cable router. 
6.Fix p2p blocking fail using Foxy.
7.Fix pppoe fixed ip issue in UK, reject our fixed ip and give a dynamic one.
8.Fix static route bug, when router under 3300 lan using 2nd subnet,   the host under the router cannot reach 3300'w WAN.
9.Fix p2p blocking fail using MSN 8.1 in Vista.
10.Fix ddns issue, fail to update IP for China ISP redirect advertisement page.
11.Fix using pppoa line with vigor100 bug.
12.Fix NAT loopback issue, client under lan but not 3300's lan subnet    (using static route to another router under 3300's lan) cannot access server     under 3300 using port redirection. 
13.Fix port redirection issue, set a rule to a host, the source port of the host be changed through NAT.
14.Fix ipsec ceasation, dial from host to lan client more than 12 using vpn tool SSH Sentinel.
15.SIP use intercall while Network failed. When Network failed, SIP using extra speed dial to make call instead of using Proxy Server.
 

Firmware Version : 2.5.7.1   / Issue 2.5.7.1
Changes Since Firmware 2.5.7
----------------------------

[New features]
1. Add bandwidth limititation function.
2. Add IP Bind to Mac function, the algorithm is same with Vigor 2xxx.
3. Add port range and source port fields for QoS feature.
4. Add IP Alias function in PPPoE mode.
5. When management port is enabled, check if VID value is set in 802.1Q VLAN
6. Add "Round Robin" ring option in VoIP Group settings.

[Improved issues]

1. Improve robustness of DDNS server registration mechanism
2. Enable physical DMZ access from LAN clients
3. Improve DHCP over IPSec operation
4. Correct QoS issue while using Outgoing/Incoming with IPSec. 


Firmware 2.5.7 (First UK Release) - Release Notes:
--------------------------------------------------

[New features]

1. Add SSH remote management function.
2. Add static DHCP function.
3. Implement IP routing function by using multiple WAN interfaces
4. Add physical DMZ function in WAN interface.
5. Add an option to turn on or turn off for management in http, telnet and SSH functions.
6. Add an option "block" or "allow" to match key words in URL Filter web page.
7. Add LFI(Link Fragmentation and Interleaving) with using MTU in QoS.
8. Add tag-based VLAN with multiple LAN interfaces.
9. Add the direction of DMZ and VPN options in IP Filter function.
10. Add encryption without authentication proposal in VPN-IPSec.
11. Add NAT Traversal of IPSec function.
12. Allow "Accept all proposal" IPSec Phase1/2 Proposals
13. Add Single Codec function in VoIP, it can be disable or enable.
14. Add line polarity reversal when callee answer the phone.
15. Add Authentication ID in VoIP protocol.
16. Add sip message log, in the CLI \voip>siplog

[End of File] 

