**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.2.2 (Formal Release)
    Release Date		: 24th November 2016
    Build Date			: 1st November 2016
    Revision			: r6620
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************
IMPORTANT NOTE: Do not upgrade directly from 1.0.5 (and earlier) to 1.2.2.
Due to differences in the Web UI and functionality the router MUST first be
upgraded to at least 1.0.7.1 prior to upgrading to 1.2.2

Upgrade your router to Version 1.0.7.1 or later first, and afterwards upgrade the router
to Version 1.2.2

[New Features]
None.

[Improvement]
1.	FTP connections in Active mode were not passed correctly through NAT
2.	When using [Diagnostics] > [Data Flow Monitor] > Packet Monitor, results could not be filtered by Host
3.	Resolved an issue that could cause higher than normal memory usage with some router configurations
4.	When configuring a User Management profile for VPN with MOTP enabled, it could not be saved without entering a password
5.	TTL values were reported incorrectly in the [Diagnostics] > [Session Table]
6.	Improved connectivity for Mac OS X SmartVPN clients

[Known Issue]
1.	High Availability - Updating from a firmware version <=1.1.0.2: Due to significant changes to High Availability functionality, existing HA configuration will be cleared during the update process and it will be necessary to reconfigure High Availability after the update
2.	Disable "Force IPsec with L2TP" option in [VPN and Remote Access] > [PPP General Setup] to allow a standard L2TP tunnel, otherwise the L2TP server will allow L2TP with IPsec only
3.	F/W 1.2.0 onwards Changes the behaviour of the IP Filter. After upgrade some IP Filter rules may need to be reconfigured. Please read the "Filter Rule Actions" segment of this guide for more information on the changes: http://www.draytek.co.uk/support/guides/kb-3900-ipfilter-basics
4.	Vigor2960 models with MXIC flash memory cannot be downgraded to firmware prior to 1.2.0.
Check the flash memory type with the CLI command "status system":
Model : Vigor2960
Hardware Version : 1.0 (M) <----- (M) suffix indicates MXIC Flash memory
Hardware Version : 1.0 <--------- no suffix indicates Samsung Flash memory, can be downgraded if required


**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.2.1 (Formal Release)
    Release Date		: 30th August 2016
    Build Date			: 27th July 2016
    Revision			: r6367
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************
IMPORTANT NOTE: Do not upgrade directly from 1.0.5 (and earlier) to 1.2.1.
Due to differences in the Web UI and functionality the router MUST first be
upgraded to at least 1.0.7.1 prior to upgrading to 1.2.1

Upgrade your router to Version 1.0.7.1 or later first, and afterwards upgrade the router
to Version 1.2.1

[New Features]
1.	The router's Online Status can display "Remote DSL" information from a Vigor 130 or Vigor 120v2 modem connected to the router's WAN ports
2.	Support WAN Load Balance by Session, configured in [Routing] > [Default Route], the default is IP-based Load Balancing
3.	[Certificate Management] > [Trusted CA Certificate] now supports "Build RootCA" to self-sign certificates
4.	Packet Monitor facility added to [Diagnostics] > [Data Flow Monitor] to capture WAN/LAN packets and download as a .pcap file
5.	Web Content Filter Query Server can now be specified in [Objects Setting] > [Web Category Object] > [Query Server] tab

[Improvement]
1.	Efficiency improvements to NAT mechanisms
2.	SSL VPN supports Idle Timeout and Reconnect
3.	APP-Enforcement Signature updated to improve handling of:
		IM-Google Hangouts
		Protocol-DNS
		HTTP
		SSL/TLS
		Tunnel-Ultrasurf
		VoIP-RC
		WebHD-HTTP_Upload
4.	Web interface response time improved when displaying large numbers of Profiles (User Profile, IP Objects, etc)
5.	Improved TCP SYN+FIN filtering mechanism
6.	Auto DDoS defense added to reduce CPU load if DDoS occurs


[Known Issue]
1.	High Availability - Updating from a firmware version <=1.1.0.2: Due to significant changes to High Availability functionality, existing HA configuration will be cleared during the update process and it will be necessary to reconfigure High Availability after the update
2.	Disable "Force IPsec with L2TP" option in [VPN and Remote Access] > [PPP General Setup] to allow a standard L2TP tunnel, otherwise the L2TP server will allow L2TP with IPsec only
3.	F/W 1.2.1 Changes the behaviour of the IP Filter. After upgrade some IP Filter rules may need to be reconfigured. Please read the "Filter Rule Actions" segment of this guide for more information on the changes: http://www.draytek.co.uk/support/guides/kb-3900-ipfilter-basics
4.	Vigor2960 models with MXIC flash memory cannot be downgraded to firmware prior to 1.2.0.
Check the flash memory type with the CLI command "status system":
Model : Vigor2960
Hardware Version : 1.0 (M) <----- (M) suffix indicates MXIC Flash memory
Hardware Version : 1.0 <--------- no suffix indicates Samsung Flash memory, can be downgraded if required


**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.2.0 (Formal Release)
    Release Date		: 4th December 2015
    Build Date			: 27th November 2015
    Revision			: r5714
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************
IMPORTANT NOTE: Do not upgrade directly from 1.0.5 (and earlier) to 1.2.0.
Due to differences in the Web UI and functionality the router MUST first be
upgraded to at least 1.0.7.1 prior to upgrading to 1.2.0

Upgrade your router to Version 1.0.7.1 or later first, and afterwards upgrade the router
to Version 1.2.0

[New Features]
1.	CPU, Memory, Traffic Tx/Rx usage added to [Notification Object], configured under Advanced Setting tab
2.	[Configuration Backup] > [Analysis] displays details of router configuration on one page
3.	Auto Firmware Upgrade and Auto Firmware Patch now available to simplify update process
4.	[User Management] > [Web Portal] new features:
	Can use SMS as an authentication method (requires internet SMS provider configured)
	Option to block mobile devices if required
	Customise login & background images in Portal Page Setup 
5.	MAC/Vendor Object now supported for use with IP Filter
6.	SMB Server now available under [USB Application] menu for file sharing of connected USB storage
7.	Now supports SHA2_256 for IPsec VPN tunnel authentication
8.	SSL VPN port can now be configured as a separate port from HTTPS Management under [System Maintenance] > [Access Control]
9.	Service Usage Monitor added to [Diagnostics] > [Data Flow Monitor] to observe data usage of specified protocols

[Improvement]
1.	Improvements to the design and functionality of [Applications] > [High Availability]
2.	Corrected an issue with Port Redirection which could occur after upgrading to 1.1.x firmware
3.	[Firewall] > [Filter Counter] indicates how many sessions have matched each rule
4.	General improvements to [Firewall] menus and syslog output
5.	Improvements to HTTPS filtering when using Web Content Filtering
6.	Specify Remote IP / Host Name to limit Remote Dial-In VPN connections to that WAN IP / Hostname only
7.	Bandwidth Limit can now apply to PPTP Remote Dial-In VPN clients
8.	[Diagnostics] > [ARP Cache Table] now has an option to quickly create an IP Object for listed IP address
9.	Supports Suffix Type in IPv6 Object configuration
10.	Time Schedule in Filter Rules can now force sessions to clear when the schedule takes effect
11.	Spotify can now be blocked with the Application Filter
12.	Can specify which WAN interfaces can be used for remote management
13.	Improvements to Traffic Graph and Data Flow Monitor
14.	QoS Class was not displayed in the Session Table
15.	Support for "esendex" SMS Provider
16.	Custom SMS Provider option to define API settings manually for SMS providers not listed

[Known Issue]
1.	Due to significant changes to High Availability functionality, existing HA configuration will be cleared during the update process and it will be necessary to reconfigure High Availability after updating to 1.2.0
2.	Vigor2960 models with MXIC flash memory cannot downgrade to previous firmware versions. 
Check the flash memory type with the CLI command "status system":
Model : Vigor2960
Hardware Version : 1.0 (M) <----- (M) suffix indicates MXIC Flash memory
Hardware Version : 1.0 <--------- no suffix indicates Samsung Flash memory, can be downgraded if required
3.	Disable "Force IPsec with L2TP" option in [VPN and Remote Access] > [PPP General Setup] to allow a standard L2TP tunnel, otherwise the L2TP server will allow L2TP with IPsec only
4.	F/W 1.2.0 Changes the behaviour of the IP Filter. After upgrade some IP Filter rules may need to be reconfigured. Please read the "Filter Rule Actions" segment of this guide for more information on the changes: http://www.draytek.co.uk/support/guides/kb-3900-ipfilter-basics


**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.1.0.2 (Formal Release)
    Release Date		: 9th September 2015
    Build Date			: 29th August 2015
    Revision			: r5461
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************
IMPORTANT NOTE: Do not upgrade directly from 1.0.5 (and earlier) to 1.1.0.2.
Due to differences in the Web UI and functionality the router MUST first be
upgraded to at least 1.0.7.1 prior to upgrading to 1.1.0.2

Upgrade your router to Version 1.0.7.1 or later first, and afterward upgrade the router
to Version 1.1.0.2

[New Features]
None.

[Improvement]
1.	Corrected an issue that could cause Port Redirection to not work after upgrading the firmware from 1.0.9 or earlier
2.	Syslog to USB was not writing to USB after restarting the router
3.	It was not possible to modify the max failed Telnet Login attempts before the router bans the IP
4.	Netbios names were not displaying in the ARP cache table correctly
5.	Improvements to certificate handling for the router's HTTPS interface
6.	DNS Suffix (DHCP Option 15) support added for remote dial-in VPN clients
7.	Upgraded OpenSSL to 0.9.8zg for security updates
8.	Resolves a WAN connectivity issue that could occur after after an extended duration

[Known Issue]
1.	Disable "Force IPsec with L2TP" option in [VPN and Remote Access] > [PPP General Setup] to allow a standard L2TP tunnel, otherwise the L2TP server will allow L2TP with IPsec only

**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.1.0.1 (Formal Release)
    Release Date		: 31st July 2015
    Build Date			: 16th July 2015
    Revision			: r5291
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************
IMPORTANT NOTE: Do not upgrade directly from 1.0.5 (and earlier) to 1.1.0.1.
Due to differences in the Web UI and functionality the router MUST first be
upgraded to at least 1.0.7.1 prior to upgrading to 1.1.0.1

Upgrade your router to Version 1.0.7.1 or later first, and afterward upgrade the router
to Version 1.1.0.1

[New Features]
None.

[Improvement]
1.  Resolved issue that could cause PPTP Remote Dial In throughput reduction
2.  Corrected issue that could cause Port Redirection to not work after upgrading the firmware from 1.0.9 or earlier
3.  Corrected NAT Loopback issue for PPTP dial-in user accessing WAN IP alias
4.  IPv6 could not get public IP via DHCP IA PD.
5.  LAN to LAN for SSL VPN would not re-connect automatically after VPN disconnection
6.  Incorrect remote IP address displayed for SSL VPN in connection history
7.  SNMP deamon correction
8.  Corrected issue that could prevent Policy route via NAT from working
9.  Corrected issues that could prevent TR-069 from working in some configurations
10. Change profile number for Policy Route to 120, and for Static Route to 200

[Known Issue]
1. You need to disable "Force IPsec with L2TP" options for pure L2TP tunnel in [VPN and Remote Access] > [PPP General Setup].
 
**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.1.0 (Formal Release)
    Release Date		: 19th June 2015
    Build Date			: 6th June 2015
    Revision			: r5142
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************
IMPORTANT NOTE: Do not upgrade directly from 1.0.5 (and earlier) to 1.1.0.
Due to differences in the Web UI and functionality the router MUST first be
upgraded to at least 1.0.7.1 prior to upgrading to 1.1.0.

Upgrade your router to Version 1.0.7.1 or later first, and afterward upgrade the router
to Version 1.1.0.

[New Features]
1.	SSL VPN LAN to LAN tunnel (Supported from DrayTek Vigor 2960 / 3900 1.1.0 firmware and Vigor 2860 / 2925 3.8.x firmware).
2.	Internal RADIUS server under [User Management] > [RADIUS].
3.	APP Enforcement supported app list added under [Objects Settings] > [APP Support List].
4.	Added auto/manual APP Signature Upgrade setting page in [System Maintenance] > [APP Signature Upgrade].
5.	[System Maintenance] > [Access Control] Improvements:
	Validation Code in Access Control tab to improve web admin security;
	Fail to Ban setting page to automatically block IP addresses after failed login attempts;
	Access Barrier setting page to protect router services (WUI, FTP etc) from brute force attack.
6.	Added Switch Rate Limit setting page in [Firewall] > [Dos Defense].
7.	Added [NAT] > [Connection Timeout] to allow altering the session timeout of different traffic types i.e. TCP, UDP etc
8.	Wake on LAN can now operate on a schedule by configuring profiles in [Applications] > [Wake on LAN] > [Schedule Wake on LAN]
9.	[Diagnostics] > [MAC Address Table] added.
10.	[Diagnostics] > [User Status] added, to show PPPoE / Web Portal / VPN / SSL Proxy users in one location.
11.	[LAN] > [LAN DNS] now supports wild-card strings and CNAME records for individual LANs using the Specified LAN option.
12.	[Routing] > [Policy Route] Improvements:
	Priority options (Normal, High, Top) for more flexible routing.
	Country Objects as destination addresses.
	Failover options for target IP ping failure.
13.	Support for Multicast via VPN.
14.	Router's web interface can now notify of new firmware upgrades available.

[Improvement]
1.	Improved DDoS protection.
2.	SSL VPN settings now available under [VPN and Remote Access] > [PPP General Setup].
3.	PPTP Dial-In VPN Profile (LAN to LAN) now supports multiple remote subnets.
4.	LDAP/RADIUS support for the router's SSL Proxy facility.
5.	[User Management] > [Web Portal] > [Portal Page Setup] now supports uploading an HTML file as the bulletin message.
6.	Packet Inspection settings added under [Firewall] > [Filter Setup] > [Default Policy]
7.	[User Management] > [User Profile] > [Apply All] improved to allow multiple choice.
8.	Port Statistics now shown under [Diagnostics] > [Traffic Statistics].
9.	Session Information added to [Diagnostics] > [Traffic Graph].
10.	Vendor Information added to [Diagnostics] > [ARP Cache Table].
11.	Daily / Period timout settings added to Web Portal under [User Management] > [Web Portal] > [General Setup].
12.	Bind IP to MAC can now be applied to specific subnets.
13.	Supported added for VPN routing through GRE over IPSec tunnel (VPN Trunk).
14.	Keep VPN Setting option added to [Central VPN Management] > [CPE Management].
15.	Alert interval of temperature sensor now configurable under [USB Application] > [Temperature Sensor] > [General Setup].
16.	The router could not use a DNS server located on the LAN for DNS queries under some circumstances.
17.	Traffic was unable to pass between LAN and PPPoE server clients.
18.	Web Content Filter category selection page improvements.
19.	IP Filter now shows a counter display for matched packets.

[Known Issue]
1. You need to disable "Force IPsec with L2TP" options for pure L2TP tunnel in [VPN and Remote Access] > [PPP General Setup].
 
**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.9.1 (Formal Release)
    Release Date		: 16th February 2015
    Build Date			: 30th January 2015
    Revision			: r4763
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]
None.

[Improvement]
1. The IGMP Proxy feature's compatibility with some ISPs that use PPPoE has been improved.
2. Support for the Bandluxe C330 USB 3G modem.
3. SSL VPN now changes tunnel MTU in relation to the WAN MTU.
4. PPTP Dial-In User VPN connections could not access the internet under some circumstances.
5. Policy Route was not working with return path traffic.
6. The IPsec option "Auto Dial Out if WAN1 Down" was still taking effect after being disabled in the WUI.
7. The router's memory usage was higher than normal when using the Data Flow Monitor.
8. The Access Control List was not working correctly under some circumstances.
9. Improvements to ensure immunity to Ghost/CVE-2015-0235

[Known Issue]

1. You need to disable "Force IPsec with L2TP" options for pure L2TP tunnel in VPN and Remote Access >> PPP General Setup.

**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.9 (Formal Release)
    Release Date		: 29th October 2014
    Build Date			: 21st October 2014
    Revision			: r4394
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]
1. Improve SSL VPN throughput for SSL VPN tunnel mode with Smart VPN Client 4.3.1 or later.
2. Supports USB 4G/LTE. Check [USB]-[Modem support list] in the router's web interface for details.
3. Supports USB disk /FTP server.
4. Supports saving Syslog to USB disk.
5. Supports Policy Route (replacing Load Balance Rule and Address Mapping menus).

[Improvement]

1.  Corrected: Connection request notifications from Vigor ACS were not authenticated
2.  Corrected: Can't establish IPv6 static connection.
3.  Improved: IPSec VPN tunnel can now be configured to pass or block NetBios packets.
4.  Improved: Allow downloading/uploading private key (for Host to LAN VPN by X.509).
5.  Improved: Show the VPN Type/Form fields on VPN History web page.
6.  Improved: Handling for Duplicated Routes (with Static Route Metric). When the static route metric is <=10, the priority of that static route will be greater than a VPN route.
7.  Improved: Support QoS for VoIP traffic from LAN.
8.  Improved: Support "Ping to Keep Alive" feature for detecting whether an IPsec tunnel is able to pass traffic
9.  Improved: Support WAN Port and IP Alias options for PPTP Dial Out connection.
10. Improved: Support RFC 4638 (accommodating an MTU/MRU larger than 1492 for PPPoE protocol WAN connections).
11. Improved: Added STUN server option to TR-069 settings.
12. Improved: Added Jumbo Frame setting under [LAN]-[Switch]-[Jumbo Frame] to edit Maximum Frame size.
13. Improved: Added a "Clear" button for the DDNS settings page.
14. Improved: Bind IP to MAC can now export or import a list of IP / MAC addresses.
15. Improved: [Sytem Maintenance] - [Access Control] can now be configured to accept pings from the WAN on specified WAN interfaces.
16. Improved: Added “OVH” as service provider for DDNS setting.
17. Improved: Supports Range-to-many Port Redirection.
18. Improved: Improve login page customization for Web Portal setup.
19. Improved: Change mechanism of deleting objects.
20. Improved: Upgrade OpenSSL to 0.9.8zc for SSLv3 Fallback (CVE-2014-3566) protection.


**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.8.2 (Formal Release)
    Release Date		: 14th July 2014
    Build Date			: 13th June 2014
    Revision			: r3968
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]

None

[Improvement]

1. Update OpenSSL to 0.9.8za
2. WCF (Web Content Filter) updated for Service Name from Commtouch to Cyren.
3. Resolved some HA (High Availability) issues
4. Corrected issue with DDNS failover 3G WAN

[Known Issue]
1. VPN Trunk tunnel doesn't work well when the profile name is more than 15 characters.
2. You need to disable "Force IPsec with L2TP" options for pure L2TP tunnel in VPN and
Remote Access >> PPP General Setup.


**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.8.1 (Formal Release)
    Release Date	: 17th June 2014
    Build Date		: 22th May 2014
    Revision		: r3863
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]

None

[Improvement]
Web User Interface Change
1.  PPTP connection stability.
2.  Web Portal stability.
3.  Remove management port setting which may occupy port redirection.
4.  Improve the stability of High Availability function.
5.  Add telnet timeout if not login in 60 seconds.
6.  CPU usage is too high when data flow monitor is enabled.
7.  SSL VPN client fixed
8.  A problem of WCF license occurred when HA is enabled.
9.  CVM can't perform configuration backup.
10. NAT Loopback to LAN More Subnet doesn’t work.
11. DNS for PPTP Remote dial-in is not assigned according to the LAN Profile.
12. Reboot with Customized Configurations bug.
13. When firewall default policy (block) is used, HTTP is still available for access.
14. Web portal still supports URL redirect when login mode is disabled.
15. Packet count error when PPTP acceleration is enabled.
16. mOTP User profile cannot be saved without Password.
17. WAN Priority Bits doesn’t work.
18. An error occurred in time object.
19. An error occurred in WAN >> Switch mode >> double tag.


**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.8 (Formal Release)
    Build Date		: 10th March 2014
    Revision		: r3548
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************
[New Features]

1.  Same WAN VLAN ID can be used in different WAN interfaces. (WAN >> General
Setup Mode: Advance, Switch Mode: Double Tag)
2.  QoS for multiple WANs.
3.  SNMP v3 Support
4.  Support country block for Firewall.
5.  Support WCF white list.
6.  Support LAN DNS server.
7.  BGP routing protocol Support
8.  SSL VPN tunnel mode (up to 20 tunnels).
9.  Support Web Portal and Hotspot (Guest profile) in User Management.
10. Support PPTP acceleration for PPTP WAN/Remote Dial-in/LAN to LAN (90Mbps with MPPE, 400Mbps without MPPE).
11. Support QoS retag option.
12. Support VPN dial-out failover if WAN disconnected.
13. Support VPN LAN to LAN for overlap/duplicate subnets.
14. High Availability Support.
15. Display the last UP/DOWN log of VPN profile.
16. Add default policy for Firewall and default block policy can be applied.
17. Add IPv6 firewall settings.
18. Add DNS object.
19. Add a remote capture telnet command (rc), for traffic monitor and wireshark remote
capture.
20. Add front panel and VPN status on the dashboard.


[Improvement]

Web User Interface Change
1.  Change the menu item “User Management>>General Setup” into “User
Management>>Web Portal”.
2.  Move IP Routing from LAN to Static Route and rename as LAN/WAN Proxy ARP.
3.  Move Inter-LAN Route from LAN>>Static Route to LAN>>General Setup.
4.  Move status page to the first tab of each function menu.

Others
5.  Support RADIUS, LDAP, Local authentication in User Management.
6.  Support NAT option for IPsec LAN to LAN.
7.  Support LDAP profile in Firewall.
8.  Support ratio configuration for VPN Load Balancing.
9.  Port number setting for Access Control in WAN IP alias can be passed to LAN
by default.
10. Notification object can be recorded on Syslog through the configuration on
Applications>>SMS/Mail Alert Service page.
11 Support Local/RADIUS/LDAP authentication for PPTP/L2TP/PPPoE server at
the same time.
12. Change the priority of Inter-LAN route, that IP filter can do further control.
13. Support connection failover for TR-069.
14. Display router name in web page title.
15. IPsec VPN dial-in connection with all WANs is supported in default.
16. Support RFC3021.
17. Combine IM/P2P/Protocol object to App Object for blocking more Apps.
18. The number of Management Access Control List is increased up to 16.
19. Support peer identity for IPsec RSA authentication.
20. Support password encode option for configuration backup.
21. Support more special characters in username for user profile.
22. The number of SSL web proxy/VNC/RDP profile is increased up to 30.
23. Support customized DDNS.
24. Support acceleration of fragmented UDP packets (maximum 1628 bytes).
25. Support DHCP option 95 (LDAP server), 161(FTP server), and 162 (File path)
for DHCP server.
26. Support more subnet DHCP servers in Bind IP to MAC.
27. Support DHCP relay over LAN/Non-Direct-Connected LAN.
28. Support DHCP relay settings for PPTP/L2TP/PPPoE.
29. Support open port to the host in remote VPN network.
30. Default route cannot work well when two WAN IPs are in the same IP network.


**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.7.1 (Formal Release)
    Release Date        : 13th November 2013
    Build Date		: 12th November 2013
    Revision		: r3067
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]
None.

[Improvement]
1.  Support USB-WAN for WAN Profile under the Setting tab in Application>> Dynamic DNS.
2.  Modify the mechanism for IP filter, "if no further match" action.
3.  Add a subnet mask setting, 255.255.255.254, for WAN IP configuration.
4.  Added option disable negotiation for Fiber WAN under the Interface tab in WAN>>Switch.
5.  QoS IP rule can apply the packets passing through both Local IP and Remote IP.
6.  ‘space’ special character can be used in the username for LDAP
7.  Improved PPTP service mechanism for multiple simultaneous LAN to LAN dial-ins
8.  Corrected: Can not block / unblock some IPs on Diagnostics>>Data Flow Monitor.
9.  Corrected issue with ICMP packets larger than 8138 bytes over IPSec LAN to LAN tunnel.
10. Corrected: The user can not access Internet when QoS queue weight is set as “0”.
11. Corrected: Lower the priority of Inter-LAN routing function.
12. Corrected: LAN DHCP packets do not respond while LAN DHCP Server is OFF.
13. Corrected: Can’t accept L2TP VPN from none default route WAN.
14. Corrected: RADIUS client (Vigor router) sends wrong NAS IP address (127.0.0.1).
15. Corrected traffic status of DHCP over IPsec in VPN Connection Management.
16. ARP detection may fail when WAN TX traffic is full.
17. Corrected: SMS can't be sent out when L2TP over IPsec is up and down.

[Known Issue]
1.  VPN Trunk tunnel doesn't work well when the profile name is more than 15 characters.
2.  You need to disable "Force IPsec with L2TP" options for pure L2TP tunnel in [VPN and
Remote Access]>[PPP General Setup]

**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.7 (Formal Release)
    Build		: r2733
    Release Date        : 2nd Sept 2013
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]
1.  Support Central VPN Management (CVM). Up to 12 devices can be managed.
2.  Support 3G backup/load balance.
3.  Support inbound load balance.
4.  Support VPN Trunk failover mode.
5.  Support PPPoE quota setting and MAC address filter.
6.  Support USB temperature sensor. http://www.draytek.co.uk/products/usb-thermometer.html
7.  Support SMS, Email Alert and Notification object profiles for WAN/VPN connection and USB temperature sensor.
8.  Support Bridge VLAN function for LAN/WAN bridging.

[Improvement]
1.  Improved: Support SmartMonitor users up to 200.
2.  Improved: VPN Trunk throughput and stability.
3.  Improved: By default disable insecure SSL Encryption Key Algorithms
4.  Improved: Support DHCP relay on VPN.
5.  Improved: QoS redesigned
6.  Improved: Username reported to Syslog
7.  Improved: Add option 60(Vendor ID), 61(Client ID) for WAN DHCP mode.
8.  Improved: Add default maximum session number for Session limit.
9.  Improved: Add flow control settings for Switch.
10. Improved: Add user defined options for DHCP server.
11. Improved: Improve DMZ function.
12. Improved: Add log and force update function for DDNS.
13. Improved: Add Force L2TP with IPsec policy option enabled in default.
14. Improved: Corrected causes for high CPU usage being displayed in Web UI
15. Improved: Stability in TR-069.
16. Improved: Firmware upgrade speed.
17. Fixed: Time object cannot work correctly when daylight saving is enabled.

[Known Issue]
1.  VPN Trunk tunnel doesn't work well when the profile name is more than 15 characters.
2.  You need to disable "Force IPsec with L2TP" options for pure L2TP tunnel in [VPN and
Remote Access]>[PPP General Setup]

**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.6.2 (Formal Release)
    Build		: r2215
    Release Date        : 5th July 2013
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]
None

[Improvements]
1. Resolved LAN port inter-operability issue that could cause the Vigor 2960 to disconnect from the LAN after a period of time
2. WAN re-connection could trigger VPN trunk to disconnect

**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.6.1 (Formal Release)
    Release Date        : 26th April 2013
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]
None

[Improvements]
1.  Improved the throughput among different VLANs.
2.  Add support for VPN on Alias WAN IP and IP Routing IP.
3.  Send ARP of WAN Alias IP to WAN Gateway when connected.
4.  Configuration Backup menu improved
5.  Added more parameters and improved the stability for TR-069.
6.  NAT Port Redirection Rule for FTP server didn't work when two WAN
connections are up.
7.  Customized web content message disappears after rebooting the router.
8.  VPN Trunk tunnel didn't work well when the profile name was long.
9.  Corrected display error for PPTP connection in VPN Graph on Syslog.
10. Ping to VPN remote network didn't work after clicking WAN DHCP Renew
Button via web user interface.
11. Session limit applied the incorrect limit due to error in calculating mask.
12. WAN status was up while WAN cable was unplugged and WAN detection mode
was set to None.
13. Something wrong with SNMP Set/Get Community.
14. VPN Traffic could not pass anymore while one of the VPN GRE tunnels was
disconnected.
15. Corrected DHCP renew interoperability issue with some ISPs.
16. Corrected SIP ALG
17. IPSec tunnel uptime might not reset whene tunnel disconnected and re-established
18. Corrected issue with PPTP control session that could prevent new connections.
19. A PC from remote subnet via PPTP LAN to LAN couldn't access into Internet via VPN
20. Improved handling of certain IPv6 packets.
21. Corrected Load balance error when using multiple PPPoE connection with the same gateway.


**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.6 (Formal Release)
    Release Date        : 12th December 2012
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[Improvements]
1.  Support VPN(IPsec) Routing Acceleration.
2.  Support VPN Alarm via E-mail & Syslog.
3.  Support VPN Graph for Syslog utility.
4.  Support PPPoE server for LAN PC connection.
5.  Add QQ account filter.
6.  Add LDAP/AD for VPN PPTP, L2TP authentication.
7.  URL Content Filter can block HTTPS connection by host keyword.
8.  Improved: WCF (Web Content Filter) supports HTTPS block by web category.

**********************************************************************

    Release Notes for Vigor 3900
    Firmware Version    : 1.0.5 (Formal Release)
    Release Date        : 17th August 2012
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

First Firmware Release

[END OF FILE]